ASL offers the possibility to generate code for totally different
processors. Currently, the following processor families are
implemented:

 - Motorola 68000..68030,683xx incl. math co-processor and MMU
 - Motorola DSP56000
 - Motorola/IBM MPC601/MPC505/PPC403
 - Motorola 6800, 6805, 6809, 68(HC)11, as well as Hitachi 6301
 - Hitachi 6309
 - Hitachi H8
 - Hitachi SH7000/7600
 - Rockwell 6502 and 65(S)C02
 - CMD 65816
 - Mitsubishi MELPS-740
 - Mitsubishi MELPS-7700
 - Mitsubishi MELPS-4500
 - Mitsubishi M16
 - Intel MCS-48/41
 - Intel MCS-51
 - Intel MCS-96
 - Intel 8080/8085
 - AMD 29K
 - Siemens 80C166/167
 - Zilog Z80, Z180, Z380
 - Zilog Z8
 - Toshiba TLCS-900(L)
 - Toshiba TLCS-90
 - Toshiba TLCS-870
 - Toshiba TLCS-47
 - Toshiba TLCS-9000
 - Microchip PIC16C54..16C57
 - Microchip PIC16C84/PIC16C64
 - Microchip PIC17C42
 - SGS-Thomson ST62xx
 - SGS-Thomson 6804
 - Texas Instruments TMS32010/32015
 - Texas Instruments TMS3202x
 - Texas Instruments TMS320C3x
 - Texas Instruments TMS370xxx
 - NEC uPD 78(C)1x
 - NEC uPD 75xxx (a.k.a. 75K0)

WWW: http://john.ccac.rwth-aachen.de:8000/as/
